Diagram A: Homing switch = OFF
1. Move in negative direction at high velocity until homing switch valid.
2. Move in positive direction at high velocity until homing switch invalid.
3. Move in negative direction at low velocity and stops after homing switch valid.

Diagram B: Homing switch = ON
1. Start to move at homing switch position in positive direction at high velocity until after homing switch.
2. Move in negative direction at low velocity and stops after homing switch valid.
